Out of service

W.O. Details:

Generator free end bearing was damaged. High temperature burned some of the components around.

TO BE INVESTIGATE,

TO BE QUOTE :

1-INSPECTION OF PONY MOTOR

2-CHECK AND REPLACE BEARING ( INCLUDING SUPPLY)

3-RECONDITION ECCITATION COILS

4- REBUSHING OF FREE END BEARING CASING

-QUOTE EVENTUALLY DISMOUNTLYNG COMPLETE PONY ROTOR FOR SHORE RECONDITION OF BEARING SURFACES

Da quello che ci segnalano i cuscinetti si sono rovinati e si e’ bruciata eccitazione sia rotorica che statorica .

Quindi chiedo un offerta buggettaria di ripristino

* Avvolgimento eccitazione Rotorico /Statorico
* Lavorazioni Meccaniche camere cuscinetti
* Lavorazioni sull’ asse con riporto materiali

La tua offerta sara’ confermata al momento che arrivera’ la macchina in tua officina .

Resto in attesa di tuo gentile riscontro .

Regards

|  |
| --- |
|  |
| Raffaele Avenia |
| Techical Service Responsible |
| TEFIN on behalf of: |
| Tefin |
| **Mobile:**+393201922345**Direct:**+39(0)81 19134434**Telephone:**+39 081 19134411**Fax:**+39 081 19134400**24/7:**+39 3914749709 |
| Via Ferrante Imparato, 501Complesso Genesis, 80147 Napoli |