**Ballast Pump Electric Motors**



A general scope of work follows:

• Disassemble of the electric motors.

• Opening and cleaning for inspection of the coil.

• Renewal of the insulation varnish of the coils.

• Replacement of the bearings.

• Shaft alignment check

• Painting

• Reassembly and test of pumps.